# AP05A-SD to AW06A-TKR-G draft procedure data:

**Route List:** Valves in route (reference only):  
AP05A-SD   
APVP-WT-V-515 YES  
APVP-WT-V-505 YES  
APVP-WT-V-530 YES  
AWVPB-WT-V-226 YES  
AWVPB-WT-V-225 YES  
AWVPB-WT-V-223 YES  
AWVPB-WT-V-222 YES  
AWVPB-WT-V-221 YES  
AW06A-WT-V-607 YES  
AW06A-WT-V-606 YES  
AW06A-TKR-G

**Section 5.5.3 heaters:** Replace existing data with the following:  
AP05A-WT-HTR-426 ET-202081  
APVP-WT-HTR-454 ET-202085  
APVP-WT-HTR-455 ET-202085  
APVP-WT-HTR-456 ET-202085  
AWVPB-WT-HTR-460 ET-202095

**Steps 5.17.9:** Replace existing data with the following:  
PUMP PIT 241-AP-05A  
VALVE PIT 241-AP-VP  
241-AW-B  
CENTRAL PUMP PIT 241-AW-06A

**Checklist 1:** Replace list with:  
AP05A **Jumper:** ????  
APVP **Jumper:** 5, 6, E, F  
APVP **Jumper:** 1, A, E  
AWVPB **Jumper:** ????  
AW06A **Jumper:** ????

**Checklist 3:**

**Checklist 4:**

**Checklist 5:**

**Checklist 6:**

**Checklist 7 - Tank pit/Structure Leak Detection**

**Checklist 7 - TFSPS Temperature Equipment Checks**  
AP05A-WT-TIT-429A ET-201693  
AP05A-WT-TIT-429B ET-201694  
AP05A-WT-TIT-429C ET-201695  
APVP-WT-TIT-211A ET-200801  
APVP-WT-TIT-211B ET-200802  
APVP-WT-TIT-211C ET-200803  
AWVPB-WT-TIT-221A ET-200830  
AWVPB-WT-TIT-221B ET-200831  
AWVPB-WT-TIT-221C ET-200832

**Checklist 7 - Drain Seal Assemblies:**  
PUMP PIT 241-AP-05A FLOOR DRAIN CLOSED  
VALVE PIT 241-AP-VP FDP-131 CLOSED  
241-AW-B FLOOR DRAIN CLOSED  
CENTRAL PUMP PIT 241-AW-06A FLOOR DRAIN CLOSED

**Checklist 7 - NACE Inspection:**  
241-AP-05A ET-202081  
241-AP-VP ET-202085  
241-AW-VPB ET-202095  
241-AW-06A ET-202093

**Test:** (Valve Positions Test)  
APVP-WT-V-515 OPEN   
APVP-WT-V-505 BLOCK APVP-WT-V-510  
APVP-WT-V-530 BLOCK APVP-WT-V-504  
AWVPB-WT-V-226 OPEN   
AWVPB-WT-V-225 BLOCK AWVPB-WT-V-227  
AWVPB-WT-V-223 BLOCK AWVPB-WT-V-224  
AWVPB-WT-V-222 OPEN   
AWVPB-WT-V-221 OPEN   
AW06A-WT-V-607 OPEN