# AP07A-PUMP to AP06A-TKR-E draft procedure data:

**Route List:** Valves in route (reference only):  
AP07A-PUMP  
AP07A-WT-V-107  
APVP-WT-V-617  
APVP-WT-V-607  
APVP-WT-V-608  
APVP-WT-V-606  
APVP-WT-V-616  
AP06A-WT-V-106  
AP06A-TKR-E

**Section 5.5.3 heaters:** Replace existing data with the following:  
AP07A-WT-HTR-431 ET-202083  
APVP-WT-HTR-454 ET-202085  
APVP-WT-HTR-455 ET-202085  
APVP-WT-HTR-456 ET-202085  
AP06A-WT-HTR-472 ET-202082

**Steps 5.17.9:** Replace existing data with the following:  
  
PUMP PIT 241 AP 07A  
VALVE PIT 241-AP-VP  
PUMP PIT 241-AP-06A

**Checklist 1:** Replace list with:  
 **Jumper:**   
AP07A **Jumper:** ????  
APVP **Jumper:** 23, 24, K  
APVP **Jumper:** 21, 22, D, K  
AP06A **Jumper:** ????

**Checklist 3:**

**Checklist 4:**

**Checklist 5:**

**Checklist 6:**

**Checklist 7 - Tank pit/Structure Leak Detection**

**Checklist 7 - TFSPS Temperature Equipment Checks**  
AP07A-WT-TIT-434A ET-201701  
AP07A-WT-TIT-434B ET-201702  
AP07A-WT-TIT-434C ET-201703  
APVP-WT-TIT-211A ET-200801  
APVP-WT-TIT-211B ET-200802  
APVP-WT-TIT-211C ET-200803  
AP06A-WT-TIT-477A ET-201697  
AP06A-WT-TIT-477B ET-201698  
AP06A-WT-TIT-477C ET-201699

**Checklist 7 - Drain Seal Assemblies:**  
   
PUMP PIT 241 AP 07A FLOOR DRAIN CLOSED  
VALVE PIT 241-AP-VP FDP-131 CLOSED  
PUMP PIT 241-AP-06A FLOOR DRAIN CLOSED

**Checklist 7 - NACE Inspection:**  
   
241-AP-07A ET-202083  
241-AP-VP ET-202085  
241-AP-06A ET-202082

**Test:** (Valve Positions Test)  
AP07A-WT-V-107 BLOCK AP07A-TKR-E  
APVP-WT-V-617 OPEN   
APVP-WT-V-607 BLOCK APVP-WT-V-615  
APVP-WT-V-608 BLOCK APVP-WT-V-618  
APVP-WT-V-606 BLOCK APVP-WT-V-620  
APVP-WT-V-616 OPEN