# AP05A-PUMP to AW02A-WT-TKR-101-2 draft procedure data:

**Route List:** Valves in route (reference only):  
AP05A-PUMP  
AP05A-WT-V-105  
APVP-WT-V-615  
APVP-WT-V-607  
APVP-WT-V-608  
APVP-WT-V-606  
APVP-WT-V-620  
APVP-WT-V-610  
APVP-WT-V-807  
AW02A-WT-V-115  
AW02A-WT-V-114  
AW02A-WT-V-116  
AW02A-WT-V-118  
AW02A-WT-TKR-101-2

**Section 5.5.3 heaters:** Replace existing data with the following:  
AP05A-WT-HTR-426 ET-202081  
APVP-WT-HTR-454 ET-202085  
APVP-WT-HTR-455 ET-202085  
APVP-WT-HTR-456 ET-202085  
AW02A-WT-HTR-463 ET-202087

**Steps 5.17.9:** Replace existing data with the following:  
PUMP PIT 241-AP-05A  
VALVE PIT 241-AP-VP  
CENTRAL PUMP PIT 241-AW-02A

**Checklist 1:** Replace list with:  
AP05A **Jumper:** ????  
APVP **Jumper:** 23, 24, K  
APVP **Jumper:** 21, 22, D, K  
APVP **Jumper:** 13, N, C  
AW02A **Jumper:** ????  
AW02A **Jumper:** K, V, Y, 2

**Checklist 3:**

**Checklist 4:**

**Checklist 5:**

**Checklist 6:**

**Checklist 7 - Tank pit/Structure Leak Detection**

**Checklist 7 - TFSPS Temperature Equipment Checks**  
AP05A-WT-TIT-429A ET-201693  
AP05A-WT-TIT-429B ET-201694  
AP05A-WT-TIT-429C ET-201695  
APVP-WT-TIT-211A ET-200801  
APVP-WT-TIT-211B ET-200802  
APVP-WT-TIT-211C ET-200803  
AW02A-WT-TIT-215A ET-200812  
AW02A-WT-TIT-215B ET-200813  
AW02A-WT-TIT-215C ET-200814

**Checklist 7 - Drain Seal Assemblies:**  
PUMP PIT 241-AP-05A FLOOR DRAIN CLOSED  
VALVE PIT 241-AP-VP FDP-131 CLOSED  
CENTRAL PUMP PIT 241-AW-02A FLOOR DRAIN CLOSED

**Checklist 7 - NACE Inspection:**  
241-AP-05A ET-202081  
241-AP-VP ET-202085  
241-AW-02A ET-202087

**Test:** (Valve Positions Test)  
AP05A-WT-V-105 BLOCK AP05A-WT-V-205  
APVP-WT-V-615 OPEN   
APVP-WT-V-607 BLOCK APVP-WT-V-617  
APVP-WT-V-608 BLOCK APVP-WT-V-618  
APVP-WT-V-606 BLOCK APVP-WT-V-616  
APVP-WT-V-620 OPEN   
APVP-WT-V-610 OPEN   
APVP-WT-V-807 OPEN   
AW02A-WT-V-115 OPEN   
AW02A-WT-V-114 BLOCK AW02A-WT-V-112  
AW02A-WT-V-116 BLOCK AW02A-WT-V-117